ORAMA ONE

Orama ONE is our standard minimal frame system offering a practically frameless opening from ceiling to floor. With a minimum profile width at 24mm and a maximum track visibility at 4mm, it can offer unobstructed views for any kind of building layout.

Highlights

Each sliding leaf running on at least 8 stainless steel wheels.

Trouble-free and invisible water drainage.

Two-point locking device for additional safety.

Adjustable base to overcome construction imperfections.

All parts thermally broken.

Specifications

Minimum profile facing width: 24 mm

Minimum meet-style profile facing width: 47 mm

Maximum sliding leaf height: 6,5 m

Maximum sliding leaf width: 3 m

Maximum sliding leaf weight: 1000 kg

Maximum sliding leaf area: 12 m²

Maximum fixed leaf area: 18 m²

Available in double (Omicron) or triple (Ωmega) glazing

Glass thickness: up to 36mm

Motorized function (Orama MOTOR) compatible.

Mosquito screen (Orama NET) compatible.

Certifications  
  
Uw values (depending on glass type & dimension): From 0,7 to 1,7 W/m2K

Air permeability: EN 12207 : Class 4

Resistance to rain penetration: EN 12208 – Class 7A

Resistance to wind loads: EN 12210 – Class C5

Sound insulation: up to 39 dB

Resistance to burglary: ENV 1627

Accessibility: DIN 18040 - 2